

RFID System Setup with Arduino

Using an Arduino board, jumper wires, RFID tags, and an RFID reader, this document offers a step-by-step tutorial for configuring an RFID system. This configuration enables RFID tag reading and has multiple uses, such as inventory management and access control.


# Required Components

- Arduino board (e.g., Arduino Uno) 

- Jumper wires (male-to-female and/or male-to-male)




- RFID Reader (e.g., MFRC522)



- RFID Tags (cards or key fobs)




- Breadboard (optional for easier wiring)



- USB cable for Arduino to connect to PC



- Arduino IDE installed on your computer



# Wiring Instructions

1. Connect the RFID reader to the Arduino using jumper wires as per the following:  
 - SDA (SS) → Arduino pin 10  
 - SCK → Arduino pin 13  
 - MOSI → Arduino pin 11  
 - MISO → Arduino pin 12  
 - IRQ → Not connected  
 - GND → Arduino GND  
 - RST → Arduino pin 9  
 - 3.3V → Arduino 3.3V (DO NOT use 5V as it may damage the reader)

# Software Setup

1. Open the Arduino IDE.  
2. Install the MFRC522 library:  
 - Go to Sketch > Include Library > Manage Libraries...  
 - Search for 'MFRC522' and install it.  
3. Open an example sketch:  
 - File > Examples > MFRC522 > DumpInfo  
4. Upload the sketch to the Arduino board.  
5. Open the Serial Monitor (set baud rate to 9600).  
6. Place an RFID tag near the reader and observe the output.

# Testing the Setup

The Arduino will read the UID of any RFID tag placed close to the reader after it has been uploaded. On the Serial Monitor, tag information ought to be visible. This demonstrates that your configuration is operating as intended.